Parameters used for the client (command line):

owlps-client.semistatic -i 192.168.11.254 -n 15 -t 10 -F 290

        Destination IP: 192.168.11.254
        Destination port: 9900
        Interface: 
        Delay (ms): 10
        Number of packets: 15
        Flood delay (ms): 290
        Listening port: 0
        Direction: 0
        X: 0.000000
        Y: 0.000000
        Z: 0.000000
